**Daily Calibration Log for Endo-Leak Tester (ZUTR30005) **

Endo-Leak Tester is compatible with ACMI, Fujifilm, Fuse, Olympus, Pentax, Richard Wolf & Storz endoscopes.

**Calibrate the ENDO-LEAK TESTER daily**:

1. Connect the Calibration Gauge to the Calibration Gauge Adapter.
2. Connect the Calibration Gauge Adapter to the Endo-Leak Tester.
3. Power the toggle switch on and press “RUN” to start calibration of the Endo-Leak Tester.
4. The Endo-Leak Tester is calibrated to produce air pressure at 150 mmHg. If the gauge shows **+/- 3mmHg** than the set pressure, please contact Zutron Medical.

**Month/Year:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **Serial #:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| DAY |  |  | INITIAL | COMMENTS |
| 1 | PASS | FAIL |  |  |
| 2 | PASS | FAIL |  |  |
| 3 | PASS | FAIL |  |  |
| 4 | PASS | FAIL |  |  |
| 5 | PASS | FAIL |  |  |
| 6 | PASS | FAIL |  |  |
| 7 | PASS | FAIL |  |  |
| 8 | PASS | FAIL |  |  |
| 9 | PASS | FAIL |  |  |
| 10 | PASS | FAIL |  |  |
| 11 | PASS | FAIL |  |  |
| 12 | PASS | FAIL |  |  |
| 13 | PASS | FAIL |  |  |
| 14 | PASS | FAIL |  |  |
| 15 | PASS | FAIL |  |  |
| 16 | PASS | FAIL |  |  |
| 17 | PASS | FAIL |  |  |
| 18 | PASS | FAIL |  |  |
| 19 | PASS | FAIL |  |  |
| 20 | PASS | FAIL |  |  |
| 21 | PASS | FAIL |  |  |
| 22 | PASS | FAIL |  |  |
| 23 | PASS | FAIL |  |  |
| 24 | PASS | FAIL |  |  |
| 25 | PASS | FAIL |  |  |
| 26 | PASS | FAIL |  |  |
| 27 | PASS | FAIL |  |  |
| 28 | PASS | FAIL |  |  |
| 29 | PASS | FAIL |  |  |
| 30 | PASS | FAIL |  |  |

**Please refer to the Endo-Leak Tester IFU for more details. Or contact your local distributor or Zutron Medical for further assistance: 877-343-5873**